SIKAFLEX® 11FC

Sikaflex 11FC is a fast curing one-component polyurethane sealant/adhesive with permanent elasticity.

USE

As an elastic adhesive for:

* Assembling metal framed buildings.
* Cover plates and covings.
* Light-weight construction materials.
* Acoustic ceiling tiles.
* Wood, metal or plastic window and door frames.
* Floor mouldings and door sills.

As an elastic joint sealant for:

* Sealing joints in concrete, epoxy, stone and quarry tiled floors.
* Sealing joints in roofing and guttering etc.
* Flexible draught proofing.
* Containers, water tanks and silos.
* Excellent pick resistance for applications in shop fronts, prisons, schools, public amenities and buildings.
* Bolted lap joints.
* Sealing penetrations in walls or floors for ducts, piping, etc.
* Sanitary purposes.

CHARACTERISTICS AND ADVANTAGES

* New Sikaflex 11FC will bond to well cleaned old Sikaflex 11FC.
* Excellent adhesion on all cement-based materials, brick, ceramics, metals, wood, polyurethane, epoxy, and some polyesters.
* Fast cure rate.
* High durability.
* High abrasion resistance and tear strength.
* Good weathering and water resistance.
* Non-sag on vertical joints up to 30 mm width.
* Ready for immediate use – no mixing.
* Non-corrosive.
* Can be painted over with many water, solvent and rubber-based paints (preliminary tests recommended).
* Certified for use in contact with potable water (AS4020-2005).

COLOUR

Black, Grey, White, (Japan Beige:600ml only)

PACKAGING

310 ml cartridge in cartons of 12

600 ml sausage in cartons of 20

- See more at: http://aus.sika.com/en/solutions\_products/02/02a024/02a024sa08/02a024sa08100/02a024sa08101.html#sthash.mHPOwCoV.dpuf